New settlements for ancient delocalized communities. The transfer of Canolo 1951-1955



Fig. 1. The twin village of Canolo. (Carra L. Company, 1958, drawing, 1:10,000. Aerial photographs, 1954). In the Canolo Nuovo, the developments of the first batch (48 housing units) and the second batch (32 housing units) of public housing, the kindergarten, and part of the private terraced houses are represented.

Fig. 2. Canolo Municipality, Site Plan of INA-Casa in the Schiavone Fiorentino area. Map drawn up by the surveyor Filippo Multari (ACC, Designazione di area edificatoria per la costruzione di alloggi popolari INA-Casa in contrada Schiavone fiorentino del Comune di Canolo, fascicolo Eredi technical office surveyor Pasquale Gangemi).

Fig. 3. The spatial and planimetric distribution of the eight apartment buildings in the new residential center of Canolo, with the adjacent roads. Plan 1:200 (ASRC, Fondo del Genio Civile di Reggio Calabria, serie 1.3.8 Lavori di costruzione di case popolari in 1952-1953 (3096) Canolo – Contabilità finale, busta 309, fascicolo 1).

Fig. 4. Ministry of Public Works, Office of Civil Engineering in Reggio Calabria, General plan and layouts of 48 housing units for flood victims in the Municipality of Canolo. The project is endorsed by Civil Engineering Corps, State Property, I.A.C.P., the Municipality, the construction company, the State Technical Office (Ufficio tecnico erariale), and the chief engineer of Civil Engineering Corps. Legend, general plan, typical building A (ground floor and first floor), typical building B (ground floor and first floor), and the bread oven (ASRC, Fondo del Genio Civile di Reggio Calabria, serie 1.3.17 Alluvione del 1951: Canolo 1953-1956 (4155), busta 74, fascicolo 1).

Fig.5. Project for the new residential center of Canolo. Master plan (architect F. Armogida as the designer), Regional Public Works Administration for Calabria, contracting station Civil Engineering Corps of Reggio Calabria, October 27, 1952 (ASRC, Fondo del Genio Civile di Reggio Calabria, Serie 1.3.26, Trasferimento e consolidamento abitati, Canolo).

Fig.6. The 32 housing units are distributed in 5 separate buildings with different architectural typologies (the so-called “second batch”). Attached to the “Booklet of Measurements” compiled by the Civil Engineering Corps on April 1, 1954, designer architect Franco Armogida. (ASRC, Fondo del Genio Civile di Reggio Calabria, serie 1.3.17 Alluvione del 1951: Canolo 1953-1956 (4155), busta 74, fascicolo 1).
