Figure 1. The residential buildings designed by Giuseppe Terragni in Como and Seveso. Picture at the end of the construction (for the Social Houses planned by Giuseppe Terragni in Via Anzani there are no pictures at the end of construction, AGT, photographs, Novocomum, Casa Pedraglio, Villa del Floricoltore, Villa Bianca, Casa Giuliani Frigerio – AGT, Social Houses, drawings) and current (for the buildings designed in Milan see picture 3).

Figure 2. Novocomum apartment building exteriors during the final phases of the construction (AGT, photographs, Novocomum, 08/020/C/S - 08/015/E/S - 08/030/C/S), floor plan (AGT, F5, Novocomum, drawings, 6/040/B1/S/E) and elevation (AGT, F5, Novocomum, drawings, 6/041/B2/S/E) with indications of the dimensions and arrangement of the cladding slabs of Saltrio stone basement and stairs.

Figure 3. Map of the area in the North of the historic centre of Milan, with identification of the five residential buildings designed by Terragni and Lingeri. Photographs of the buildings at the end of the constructions (AGT, photographs, Casa Rustici, Casa Ghiringhelli, Casa Toninello, Casa Lavezzari, Casa Comolli Rustici).

Figure 4. On the left, detail of the cladding slabs on the ground floor of Casa Ghiringhelli, on the right, detail of the cladding slabs of Casa Toninello in the same material.

Figure 5. Detail of the cladding with Moltasio slabs (AGT, f 4, Villa a Seveso, drawings, 39/016/C1/D/L).

Figure 6. Fig. The cladding in the prefabricated elements is already present in the first drawings. On the left, the perspective of the complete planning version of the second lot, on the right the table which represents the slabs in the front. (AGT, Casa Pedraglio, drawings, 43/001/D1/D/L, 43/019/C1/S/L).

Figure 7. Details of the cladding elements. On the left, section of the detail of the cladding slabs in relation to the window and the rolling shutter (AGT, reference); on the right, details of the prefabricated elements in the plant, elevation and section (AGT, Casa Pedraglio, drawings, 43_007_C1_D_L)

Figure 8. Laying of the cladding with marble splits AGT, photographs, 72/043/C/S, GF043C - 72/040/C/S, GF040C - 72/041/C/S, GF041C, 14/12/1939).

Figure 9. Casa Lavezzari at the end of the working site in 1937 (on the left, AGT, photographs, Casa Lavezzari), after the raising and the application of fixing bosses (Carraro, M., 2004, p. 221) and in 2019 (photo by the author).




